Skip to content

# PS2-HOME.com - PS2 Homebrew and Tools

Skip to content

## FMCB Compatible PS2 Models Chart

## FAT MODELS:

FMCB | PS2 MODEL | SIZE | CHASSIS | MOTHERBOARD | ROM | BIOS | REGION | TV SYSTEM | NOTES
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
YES | SCPH-10000 | FAT | A | GH-001 | 1.00J / v1.01J |  | Japan | NTSC-J |
YES | SCPH-15000 | FAT | A | GH-003 | v1.01J |  | Japan | NTSC-J |
YES | SCPH-18000 | FAT | A+ | GH-003 | v1.20J |  | Japan | NTSC-J | WARNING: if you install FMCB on this PS2 PHAT model, and then attempt to try this MC on these PSX-DVR models: (DESR-5000 and DESR-5700), FMCB will not work. What you need to do is install FMCB on a later PHAT model. See this topic for more details: Click Here.
YES | SCPH-18000 | FAT | AB | GH-008 | v1.20J |  | Japan | NTSC-J | WARNING: if you install FMCB on this PS2 PHAT model, and then attempt to try this MC on these PSX-DVR models: (DESR-5000 and DESR-5700), FMCB will not work. What you need to do is install FMCB on a later PHAT model. See this topic for more details: Click Here.
YES | SCPH-30001 | FAT | B/B | GH-004/005 | v1.10U |  | USA | NTSC-U | AUTO TILT motor model
YES | SCPH-30001 | FAT | C/C | GH-005/006 | v1.20U/E |  | USA | NTSC-U |
YES | SCPH-30002 | FAT | C/C | GH-005/006 | v1.20U/E |  | Europe | PAL |
YES | SCPH-30003 | FAT | C/C | GH-005/006 | v1.20U/E |  | Europe | PAL |
YES | SCPH-30004 | FAT | C/C | GH-005/006 | v1.20U/E |  | Europe | PAL |
YES | SCPH-30000 | FAT | D | GH-010 | v1.50J |  | Japan | NTSC-J | The D-Chassis (series) was the first version to support the osdmain.elf universal update file.
YES | SCPH-30001 | FAT | D | GH-010 | v1.50U |  | USA | NTSC-U |
YES | SCPH-30002 | FAT | D | GH-010 | v1.50E |  | Europe | PAL |
YES | SCPH-30003 | FAT | D | GH-010 | v1.50E |  | Europe | PAL |
YES | SCPH-30004 | FAT | D | GH-010 | v1.50E |  | Europe | PAL |
YES | SCPH-30000R | FAT | D | GH-013 | v1.50J |  | Japan | NTSC-J |
YES | SCPH-30001R | FAT | D | GH-013 | v1.50U |  | USA | NTSC-U |
YES | SCPH-30002R | FAT | D | GH-013 | v1.50E |  | Europe | PAL |
YES | SCPH-30003R | FAT | D | GH-013 | v1.50E |  | Europe | PAL |
YES | SCPH-30004R | FAT | D | GH-013 | v1.50E |  | Europe | PAL |
YES | SCPH-30000 | FAT | F | GH-013 | v1.60J |  | Japan | NTSC-J | The F-Chassis (series) has a new BGA-mounted MECHACON, Rohm RTC-IC and SANYO SF-HD7 / First model to support the CXP103049 MECHACON, the Rohm RTC IC (as well as the existing Ricoh device) and both the SONY and SANYO optical blocks. / The Japanese model doesn't seem to have the "R" in its name, as the service tool indicates that it is a "SCPH-30000".
YES | SCPH-30001R | FAT | F | GH-015 | v1.60U |  | USA | NTSC-U |
YES | SCPH-30002R | FAT | F | GH-015 | v1.60E |  | Europe | PAL |
YES | SCPH-30003R | FAT | F | GH-015 | v1.60E |  | Europe | PAL |
YES | SCPH-30004R | FAT | F | GH-015 | v1.60E |  | Europe | PAL |
YES | SCPH-30005R | FAT | F | GH-015 | v1.60 |  | Korea | NTSC | Seems to be the first model to be also released in Korea (05)
YES | SCPH-30006R | FAT | F | GH-015 | v1.60 |  | Asia | ? | Seems to be the first model to be also released in Asia (06)
YES | SCPH-30007R | FAT | F | GH-015 | v1.60 |  | Tawain | NTSC | Seems to be the first model to be also released in Taiwan (07)
YES | SCPH-35000 | FAT | D |  | v1.50J |  | Japan | NTSC-J |
YES | SCPH-35001 | FAT | D |  | v1.50U |  | USA | NTSC-U |
YES | SCPH-35002 | FAT | D |  | v1.50E |  | Europe | PAL |
YES | SCPH-35003 | FAT | D |  | v1.50E |  | Europe | PAL |
YES | SCPH-35004 | FAT | D |  | v1.50E |  | Europe | PAL |
YES | SCPH-37000 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60J |  | Japan | NTSC-J | We don't have information on the SCPH-37000, so it seems like it was only released in Japan.
YES | SCPH-39000 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60J |  | Japan | NTSC-J | There were two versions of the SCPH-39000's MECHACON. The earlier one with firmware v3.6 was released in every territory that the SCPH-39000 series appeared in, while the newer one (v3.8) was only released in Japan and in Asia. / The late Japanese and Asian models had -003GG and -403GG version numbers printed on their MECHACON devices respectively. / Unlike the older models, the SONY service tool no longer gave the option for the T487 lens... so I guess that it wasn't made to support the old KHS-400B optical blocks.
YES | SCPH-39001 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60U |  | USA | NTSC-U |
YES | SCPH-39002 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60E |  | Europe | PAL |
YES | SCPH-39003 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60E |  | Europe | PAL |
YES | SCPH-39004 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60E |  | Europe | PAL |
YES | SCPH-39005 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60 |  | Korea | NTSC |
YES | SCPH-39006 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60 |  | Asia | ? |
YES | SCPH-39007 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60 |  | Tawain | NTSC |
YES | SCPH-39008 | FAT | G | GH-017 / GH-019 / GH-022 | v1.60 |  | Russia | PAL | The SCPH-39000 series appears to be the first release for Russia (08).
YES | SCPH-50000 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Japan | NTSC-J | ROM v1.90 was the first version with support for the extended languages (Russian, Korean, Simplified Chinese and Traditional Chinese), so I guess that the releases in these regions got the consoles with ROM v1.90. / As for the J-chassis - I have seen only one photograph of it. It was a Japanese SCPH-50000NB model, so I don't know whether any other region got it. Not all of the SCPH-50000NB models were J-chassis units though. / Support for nearly all regions started with this model.
YES | SCPH-50001 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | USA | NTSC-U |
YES | SCPH-50002 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Europe | PAL |
YES | SCPH-50003 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Europe | PAL |
YES | SCPH-50004 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Europe | PAL |
YES | SCPH-50005 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Korea | NTSC |
YES | SCPH-50006 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Asia | ? |
YES | SCPH-50007 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Tawain | NTSC |
YES | SCPH-50008 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | Russia | PAL |
YES | SCPH-50009 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.90 |  | China | PAL | This was the one and only model released in mainland China, as the SCPH-50009. The Chinese sets were manufactured by SONY Wuxi and had ROM v1.90.
YES | SCPH-50010 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | ? | ? |
YES | SCPH-50011 | FAT | H/I/J | GH-023 / GH-026 / GH-029 | v1.70 / v1.90 |  | ? | ? |

## SLIM MODELS:

FMCB | PS2 MODEL | SIZE | CHASSIS | MOTHERBOARD | ROM | BIOS | REGION | TV SYSTEM | NOTES
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
YES | SCPH-70000 | SLIM | K | GH-032 / GH-035 | v2.00 |  | Japan | NTSC-J | As with any slimline console, this one had a universal DVD ROM. The BOOT ROM was also largely universal, except for the PlayStation driver. As such, this was the final model that had differing ROMs for NTSC/PAL. / Support for all regions (0-12) started with this model.
YES | SCPH-70001 | SLIM | K | GH-032 / GH-035 | v2.00 |  | USA | NTSC-U |
YES | SCPH-70002 | SLIM | K | GH-032 / GH-035 | v2.00 |  | Oceana | ? |
YES | SCPH-70003 | SLIM | K | GH-032 / GH-035 | v2.00 |  | UK | PAL |
YES | SCPH-70004 | SLIM | K | GH-032 / GH-035 | v2.00 |  | Europe | PAL |
YES | SCPH-70005 | SLIM | K | GH-032 / GH-035 | v2.00 |  | Korea | NTSC |
YES | SCPH-70006 | SLIM | K | GH-032 / GH-035 | v2.00 |  | Asia | ? |
YES | SCPH-70007 | SLIM | K | GH-032 / GH-035 | v2.00 |  | Tawain | NTSC |
YES | SCPH-70008 | SLIM | K | GH-032 / GH-035 | v2.00 |  | Russia | PAL |
YES | SCPH-70009 | SLIM | K | GH-032 / GH-035 | v2.00 |  | China | PAL |
YES | SCPH-70010 | SLIM | K | GH-032 / GH-035 | v2.00 |  | ? | ? |
YES | SCPH-70011 | SLIM | K | GH-032 / GH-035 | v2.00 |  | North America | NTSC |
YES | SCPH-70012 | SLIM | K | GH-032 / GH-035 | v2.00 |  | USA | NTSC-U |
YES | SCPH-75000 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | Japan | NTSC-J | The very first slimline console to not have a real IOP device, but the PPC emulator instead. The ROMs are entirely universal, with the visible differences being the result of software-manipulation by the IOP emulator.
YES | SCPH-75001 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | USA | NTSC-U |
YES | SCPH-75002 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | Oceana | ? |
YES | SCPH-75003 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | UK | PAL |
YES | SCPH-75004 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | Europe | PAL |
YES | SCPH-75005 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | Korea | NTSC |
YES | SCPH-75006 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | Asia | ? |
YES | SCPH-75007 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | Tawain | NTSC |
YES | SCPH-75008 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | Russia | PAL |
YES | SCPH-75009 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | China | PAL |
YES | SCPH-75010 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | ? | ? |
YES | SCPH-75011 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | North America | NTSC |
YES | SCPH-75012 | SLIM | L | GH-037 / GH-040 / GH-041 | v2.20 |  | USA | NTSC-U |
YES | SCPH-77000 | SLIM | M | GH-051 / GH-052 | v2.20 |  | Japan | NTSC-J |
YES | SCPH-77001 | SLIM | M | GH-051 / GH-052 | v2.20 |  | USA | NTSC-U |
YES | SCPH-77002 | SLIM | M | GH-051 / GH-052 | v2.20 |  | Oceana | ? |
YES | SCPH-77003 | SLIM | M | GH-051 / GH-052 | v2.20 |  | UK | PAL |
YES | SCPH-77004 | SLIM | M | GH-051 / GH-052 | v2.20 |  | Europe | PAL |
YES | SCPH-77005 | SLIM | M | GH-051 / GH-052 | v2.20 |  | Korea | NTSC |
YES | SCPH-77006 | SLIM | M | GH-051 / GH-052 | v2.20 |  | Asia | ? |
YES | SCPH-77007 | SLIM | M | GH-051 / GH-052 | v2.20 |  | Tawain | NTSC |
YES | SCPH-77008 | SLIM | M | GH-051 / GH-052 | v2.20 |  | Russia | PAL |
YES | SCPH-77009 | SLIM | M | GH-051 / GH-052 | v2.20 |  | China | PAL |
YES | SCPH-77010 | SLIM | M | GH-051 / GH-052 | v2.20 |  | ? | ? |
YES | SCPH-77011 | SLIM | M | GH-051 / GH-052 | v2.20 |  | North America | NTSC |
YES | SCPH-77012 | SLIM | M | GH-051 / GH-052 | v2.20 |  | USA | NTSC-U |
YES | SCPH-79000 | SLIM | N | GH-061 / GH-062 | v2.20 |  | Japan | NTSC-J | The thickness of the PlayStation 2 was further reduced. The expansion connector on the mainboards seem to be starting to disappear around here.
YES | SCPH-79001 | SLIM | N | GH-061 / GH-062 | v2.20 |  | USA | NTSC-U |
YES | SCPH-79002 | SLIM | N | GH-061 / GH-062 | v2.20 |  | Oceana | ? |
YES | SCPH-79003 | SLIM | N | GH-061 / GH-062 | v2.20 |  | UK | PAL |
YES | SCPH-79004 | SLIM | N | GH-061 / GH-062 | v2.20 |  | Europe | PAL |
YES | SCPH-79005 | SLIM | N | GH-061 / GH-062 | v2.20 |  | Korea | NTSC |
YES | SCPH-79006 | SLIM | N | GH-061 / GH-062 | v2.20 |  | Asia | ? |
YES | SCPH-79007 | SLIM | N | GH-061 / GH-062 | v2.20 |  | Tawain | NTSC |
YES | SCPH-79008 | SLIM | N | GH-061 / GH-062 | v2.20 |  | Russia | PAL |
YES | SCPH-79009 | SLIM | N | GH-061 / GH-062 | v2.20 |  | China | PAL |
YES | SCPH-79010 | SLIM | N | GH-061 / GH-062 | v2.20 |  | ? | ? |
YES | SCPH-79011 | SLIM | N | GH-061 / GH-062 | v2.20 |  | North America | NTSC |
YES | SCPH-79012 | SLIM | N | GH-061 / GH-062 | v2.20 |  | USA | NTSC-U |
YES | SCPH-90000 | SLIM | P | GH-070 / GH-071 | v2.20 |  | Japan | NTSC-J |
YES | SCPH-90001 | SLIM | P | GH-070 / GH-071 | v2.20 |  | USA | NTSC-U |
YES | SCPH-90002 | SLIM | P | GH-070 / GH-071 | v2.20 |  | Oceana | ? |
YES | SCPH-90003 | SLIM | P | GH-070 / GH-071 | v2.20 |  | UK | PAL |
YES | SCPH-90004 | SLIM | P | GH-070 / GH-071 | v2.20 |  | Europe | PAL |
YES | SCPH-90005 | SLIM | P | GH-070 / GH-071 | v2.20 |  | Korea | NTSC |
YES | SCPH-90006 | SLIM | P | GH-070 / GH-071 | v2.20 |  | Asia | ? |
YES | SCPH-90007 | SLIM | P | GH-070 / GH-071 | v2.20 |  | Tawain | NTSC |
YES | SCPH-90008 | SLIM | P | GH-070 / GH-071 | v2.20 |  | Russia | PAL |
YES | SCPH-90009 | SLIM | P | GH-070 / GH-071 | v2.20 |  | China | PAL |
YES | SCPH-90010 | SLIM | P | GH-070 / GH-071 | v2.20 |  | ? | ? |
YES | SCPH-90011 | SLIM | P | GH-070 / GH-071 | v2.20 |  | North America | NTSC |
YES | SCPH-90012 | SLIM | P | GH-070 / GH-071 | v2.20 |  | USA | NTSC-U |
(See Notes) | SCPH-90000 | SLIM | R | GH-072 | v2.30 |  | Japan | NTSC-J | The final version of the PlayStation 2, as we know of. The folks who deal with FMCB know that this model appeared sometime around the 3rd quarter of 2008 because the USA models had a datecode of 8C. / This ROM has no support for any system updates.
YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90001 | SLIM | R | GH-072 | v2.30 |  | USA | NTSC-U | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90002 | SLIM | R | GH-072 | v2.30 |  | Oceana | ? | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90003 | SLIM | R | GH-072 | v2.30 |  | UK | PAL | YES -- if you use this method, but you still need a modchip. - Click Here!
YES | SCPH-90004 | SLIM | R | GH-072 | v2.20 |  | Europe | PAL | In April 2018, an example of a R-chassis console with ROM v2.20 was found (hence compatible with FMCB).
(See Notes) | SCPH-90004 | SLIM | R | GH-072 | v2.30 |  | Europe | PAL | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90005 | SLIM | R | GH-072 | v2.30 |  | Korea | NTSC | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90006 | SLIM | R | GH-072 | v2.30 |  | Asia | ? | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90007 | SLIM | R | GH-072 | v2.30 |  | Tawain | NTSC | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90008 | SLIM | R | GH-072 | v2.30 |  | Russia | PAL | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90009 | SLIM | R | GH-072 | v2.30 |  | China | PAL | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90010 | SLIM | R | GH-072 | v2.30 |  | ? | ? | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90011 | SLIM | R | GH-072 | v2.30 |  | North America | NTSC | YES -- if you use this method, but you still need a modchip. - Click Here!
(See Notes) | SCPH-90012 | SLIM | R | GH-072 | v2.30 |  | USA | NTSC-U | YES -- if you use this method, but you still need a modchip. - Click Here!

## PSX-DVR MODELS:

FMCB | PSX-DVR MODEL | CHASSIS | MOTHERBOARD | ROM | BIOS | REGION | TV SYSTEM | NOTES
--- | --- | --- | --- | --- | --- | --- | --- | ---
YES | DESR-5000 | X | ? | ? |  | Japan | NTSC-J | WARNING: if you install FMCB on a PS2 PHAT SCPH-18000, and then attempt to try this MC on this PSX-DVR model, FMCB will not work. What you need to do is install FMCB on a later PHAT model. See this topic for more details: Click Here.
YES | DESR-5100 | X | XPD-001 | v1.80J |  | Japan | NTSC-J |
YES | DESR-5500 | X | ? | ? |  | Japan | NTSC-J |
YES | DESR-5700 | X | ? | ? |  | Japan | NTSC-J | WARNING: if you install FMCB on a PS2 PHAT SCPH-18000, and then attempt to try this MC on this PSX-DVR model, FMCB will not work. What you need to do is install FMCB on a later PHAT model. See this topic for more details: Click Here.
YES | DESR-7000 | X | ? | ? |  | Japan | NTSC-J |
YES | DESR-7100 | X | ? | ? |  | Japan | NTSC-J |
YES | DESR-7500 | X | ? | ? |  | Japan | NTSC-J |
YES | DESR-7700 | X | ? | ? |  | Japan | NTSC-J |

## PS2 TV MODELS:

FMCB | PS2 TV MODEL | CHASSIS | MOTHERBOARD | ROM | BIOS | REGION | TV SYSTEM | NOTES
--- | --- | --- | --- | --- | --- | --- | --- | ---
NO | PX300 | ? | ? | v2.30 |  | Europe | PAL | Only released in Europe. Sony Bravia KDL-22PX300 TV. There might be no modchip for this, but you can try launching uLaunchELF using a SwapMagic procedure.
NO | PX300-1 | ? | ? | v2.50 |  | Europe | PAL | Only released in Europe. Sony Bravia KDL-22PX300 TV. There might be no modchip for this, but you can try launching uLaunchELF using a SwapMagic procedure.

Sources:

- [TUTORIAL] [FMCB] FMCB and FHDB PS2 Models Compatibility List
- PS2Ident: List of Collected and Missing Data
- List of all PS2 retail releases worldwide
- [TUTORIAL] [PS2 HARDWARE] 4 Known methods on how to find your PS2 Model Name/Number
- [TUTORIAL] [PS2 HARDWARE] PS2 MODELS and MOTHERBOARDS
- [TUTORIAL] [FMCB] Free McBoot Installation Guide [Noobie Guide]
- [APP] FMCB Installer Updated by SP193
- [APP] Unofficial FHDB 1.93 "Noobie Package" OBT
- [APP] HWC-OSDSYS Launcher by HWNJ (Runs FMCB on 90K PS2 SLIMs w/ v2.30+ BIOS!)